MAXGRIP®
WATERPROOFING ANCHORING CEMENT FOR CONCRETE AND MASONRY

Description

MAXGRIP is a mixture of cements and selected special additives and aggregates. A pourable, cement-base, non-shrinking, quick-setting hydraulic compound.

Uses

Water/Sewer Management, Road/Rail, Construction Building/Swimming Pool Industry, Bridge Building, Councils, Heavy Industry, Mining, Steel, Defence Forces.

- Setting anchor bolts, rail posts, signposts.
- Parking meters, reinforcing rods and fixtures.
- Heavy machinery anchoring, hooks, pulleys.
- Park seats, bridge railings, partitions.
- Safety rails, hand rails, balustrades.
- Flag and light poles.

Advantages

- Quick setting - 15 minutes.
- Stronger than concrete in one hour.
- Grey Colour matching perfectly with concrete. Makes structurally sound bonds.
- Add water only - easy use.
- Waterproofs surface to which it is applied.
- Non-toxic. Odourless.
- Ideal for badly ventilated areas. Pourable.
- Contains no sulphur or Iron particles, will not oxidise.

Application

Drill holes in sound concrete large enough for head and washer. If concrete is not sufficiently sound, drill deeper. To increase the strength mushroom the base of the hole by tilting the drill. Blow or vacuum out excess dust and wet sides of hole to obtain proper bonding. Place anchor bolts, with washer in hole. Mix enough material to fill the hole, mix with clean water a pancake batter consistency in a small plastic bowl or other suitable container. Pour a little MAXGRIP in the hole and work the bolt up and down a few times to eliminate any air bubbles. Pour in balance of mix from one side to ensure even flow.
MAXGRIP will set in 15 minutes, complete cure after 60 to 90 minutes and will strength as it cures, so allow more curing time for heavy machinery and other large installations.
For cold weather installations, heat hole before usin MAXGRIP. Do not add antifreeze solutions to mixing water. Store material in a warm place.

Test Data

- Compressive strenght 7 days - 444 Kg/cm².
- Pullout strength 22 mm bolt in 80 mm hole = 109, 546 Kg/cm².
- Set time l-Vicat - 15 minutes.

Recommendations

Holesize should be 3 x the size of the bolt. This will ensure that the strength of the setting compares to the tensile strength of the mild steel bolt. Depth should be 5 x the diameter of the bolt or post.

Packaging

25 Kg. pails.
5 Kg. cans

Guarantee

The information contained in this leaflet is based on our experience and technical knowledge, obtained through laboratory testing and from bibliographic material. DRIZORO reserves the right to introduce changes without prior notice. Any use of this data beyond the purposes expressly specified in the leaflet will not be the Company’s responsibility unless authorised by us. We shall not accept responsibility exceeding the value of the purchased product.

© 2003 DRIZORO S.A. All rights reserved.