MAXLEVEL®
SELF-LEVELLING MORTAR FOR INTERIOR FLOORS TREATMENT

Description

MAXLEVEL is a hydraulic setting mortar,based on cements and a blend of special arids and synthetic aggregates. MAXLEVEL mixed with water provides a fluid mortar that levels itself without trowelling after being poured.
It is the suitable product when levelling with high performances is required for interior applications.

Uses

MAXLEVEL is the key product for levelling interior floors, being the ideal method to obtain plain surfaces.

Advantages

- Self-levelling. MAXLEVEL spreads itself, even admits pumping.
- Stress-free hardening, even in thick layers applied at once.
- Suitable application over floor heating system.
- Fast hardening, allowing pedestrian traffic after two hours of its application.

Application

Surface preparation
Remove all desintegrated materials so that only sound substrate remains. The surface must be free of dirt, dust, cement grouts, paint, grease or other foreign materials.
Mixing
Pour 5,5-6 liters of water into a clean container and add 25 Kg. of MAXLEVEL. Mix thoroughly up to 2 minutes until a homogeneous mortar without lumps is achieved.
Placing
Before pouring MAXLEVEL and according to the characteristics of the surface to be treated, it is necessary to prepare the surface as follows:

- Anhydride floors, floors of absorbing cement, concrete surfaces: Priming with MAXCRYL, 2:1 water diluted.
- Cement floors, concentrated or weakly absorbing concrete surfaces, even use ful ones (ceramics, ground, etc.): Priming with pure MAXCRYL, without diluting.

Once priming is dry, pour the fluid mortar over the base and distribute regularly, applying the thick of the layer in a single step.

Test Data

Colour : | Light Grey
Requirement : | 1,4 Kg/mē per mm. thick
Powder/water mixing rate : | Each 25 Kg. of powder needs 5,5-6 liters of water
Pot life : | 20-30 minutes
Time to allow pedestrian traffic: | 2 hours approx. for 4-5 mm. thick
Time for finishing placements: | 24 hours
Application temperature : | Higher than 5° C

Storage

12 months when stored in a cool, dry, and frost free place.

Packaging

25 Kg. sack.

Guarantee

The information contained in this leaflet is based on our experience and technical knowledge, obtained through laboratory testing and from bibliographic material. DRIZORO reserves the right to introduce changes without prior notice. Any use of this data beyond the purposes expressly specified in the leaflet will not be the Company’s responsibility unless authorised by us. We shall not accept responsibility exceeding the value of the purchased product.

© 2003 DRIZORO S.A. All rights reserved.