MAXSHEEN®
A WATERPROOF ACRYLIC COATING FOR BOTH INTERIOR AND EXTERIOR USE. IT CAN BE APPLIED OVER CONCRETE, MASONRY, RENDER, STONE, CERAMICS, PLASTER OR WOOD.

Description

MAXSHEEN is an emulsion base of copolymers in aqueous dispersion. It provides a durable coating for the waterproofing and decoration of façades and interior walls. It comes in two finishes, smooth and textured.

Uses

- Over MAXSEAL, CONCRESEAL PLASTERING and MAXQUICK in orderj to achieve the required texture and colour.
- Over concrete, masonry, render, stone, asbestos cement, plaster, wood and cork.

Advantages

- Permits walls to breathe.
- Impervious to rain water.
- Quick drying depending on the temperature and humidity.
- It is flexible. It does not crack with normal temperature changes. · Excellent resistance to stains and dirt.
- Easy to clean. Just wash with soap and water.
- Good colour range.
- Excellent colour stability.
- Non-toxic and non-flammable.
- Alkali resistant.
- Easy to apply.

Application Instructions

MAXSHEEN is packaged ready for use. Stir paint well and use exactly as it comes from the can. MAXSHEEN can be applied by brush, spray or roller. Surface preparation. The surface to be painted must be clean and free from dirt, grease and efflorecence. Lime must be completely eliminated. Application. Over concrete, masonry, render, asbestos cement and stone apply two coats. The first coat should be diluted in the ratio 1:5 of MAXSHEEN and water. This coat is applied as a primer and after 2 hours cure, a second coat of neat MAXSHEEN is applied. Over plaster. The prime coat should be prepared at 30% of MAXSHEEN to water. Painted Surfaces. Remove decayed paint, grease and dirt. In case of doubt make a test patch first. Spalled and blown render must be repaired with MAXBETON or MAXREST. Cracks and joints. Open up all suspect cracks to a minimum of 5 mm width. Back fill crack with silica sand or inert packing, before sealing flush with MAXFLEX. Then paint all surfaces uniformly with MAXSHEEN. In case of doubt, enquire first. |

Precautions

Warm weather. Wet the surface several times before applying the two coats of MAXSHEEN. If the temperature is high, we recommend the MAXSHEEN should only be applied in the shade. Cold weather. Do not apply below 5° C. Do not apply if rain is expected within a few hours of application. |

Coverage

Smooth MAXSHEEN: 0,3 - 0,5 litre/m²
Textured MAXSHEEN: 0,8-1 litre/m²
Amount will depend on the absorption rate of the surface to be treated.

Laboratory Tests

Certificates no. 84.491 and 84.492
Laboratory Chimico Merceológico. Rome. Italy.

Storage

In a covered place and avoid temperatures below 0°C. The shelf life of unopened cans is 24 months.

Packaging

20 and 5 litre cans.

Colours

16 different colours.

Pearl Gray | Buff | Brick Red | Limestone
White | Azure Bleu | Battleship | Sea Green
Cemtone | Salmon | Off White | Brown
Light Gray | Castanet | Cream | Adobe
* Orientative colours

Guarantee

The information contained in this leaflet is based on our experience and technical knowledge, obtained through laboratory testing and from bibliographic material. DRIZORO reserves the right to introduce changes without prior notice. Any use of this data beyond the purposes expressly specified in the leaflet will not be the Company’s responsibility unless authorised by us. We shall not accept responsibility exceeding the value of the purchased product.

© 2003 DRIZORO S.A. All rights reserved.