MAXURETHANE® 2C
TWO COMPONENT POLYURETHANE DECORATIVE COATING WITH PORCELAINIC FINISH

Description

Aliphatic two-component polyurethane coating. Glossy, elastic and very hard once polymerised. Highly resistant to environmental exposure and UV rays, thus providing high stability of the colour.

Uses

- Exterior decorative finish, with excellent performance against weathering.
- Chemical protection, anti-corrosion and structural protection in structures, tanks, floors, etc.
- Topcoat for exterior multilayer systems, whether epoxy or polyurethane type.

Advantages

- Porcelainic finish.
- Stable against chemical aggression and exposure to weathering.
- Great durability.
- Excellent adhesion to the substrate.
- Very resistant to abrasion.
- Non toxic.

Application

Preparation of the substrate. Prior to the application of the product the surface must be dry and free of dust, grease, etc. Apply a primer coat consisting of MAXURETHANE 2C diluted with about 10% to 15% of total weight with MAXURETHANE 2C SOLVENT or MAXURETHANE PRIMER as an option.

Mixing: Stir thoroughly the content of component A container, using a DRY and CLEAN spatula. To apply by spraying it is recommended to add the solvent to component A, in the desired ratio as a proportion of the total amount of the mix (A+B). Pour component B into component A (already diluted or not) container. Stir well to achieve a perfect and homogeneous mix of both components. Due to the influence of the solvents, it is never advisable to use any solvent other than MAXSOLVENT K9.

Placing: In order to achieve a uniform finish, it is advisable that the application be done preferably by spraying gun, applying two coats, with the first one being diluted with MAXURETHANE SOLVENT.

Cautions

Caution: Apply outdoors or with adequate ventilation. Solvents included in MAXURETHANE 2C evaporate very slowly, as in any other macromolecular-type coatings. It is recommended to provide good ventilation, even after its correct application and after it shows the tack-free drying. This will become a must in enclosed spaces or in areas with difficult natural ventilation.

MAXURETHANE 2C is a flammable compound. During its application, standard fire protection precautionary measures should be adopted, usual for this type of products during application. Please refer to the Safety Data Sheet for further information. When preparing and applying on site do not work without adequate safety goggles and rubber gloves, nor near any ignition sources. If the product comes in contact with the eyes rinse thoroughly with clean water without scrubbing. See a doctor if the irritation continues.

Presentation

Supplied in sets 1, 5 and 25 kg.

Colours

See chart. Other colours upon request.

RAL 9003 | Ref. 952 | RAL 5015
RAL 7001 | RAL 3001 | RAL 6011

Note: Printed colours are indicative.

Storage

Twelve months for component A and six months for component B in their original unopened container, in a dry cool place and protected from frost.

Technical Data

Components | Two components
Mixing ratio | A: B 4:1
Recommended solvent | MAXURETHANE 2C SOLVENT
% Solids in volume | 55.04+/-0.5%
Specific weight | 1.29+/-0.05
Time for initial reaction | 15 min.
Pot life depending on colour at 20ºC | 8 - 24 hours
Dust-free drying time (20ºC 65% RH) | 1.5 hours
Tack-free drying time (depending on temp and RH) | 4 - 6 hours
Time to paint over | 6 - 12 hours
Yield sq./ litre | 13.8
Yield sq. / kg. | 10.6
Recommended dry film thickness | 40 microns

Characteristics of the dry film

- Resistance to saline environment : Longer than 1500 hours
- Toxicity: Non toxic. Odour and taste free.
- Physical and chemical resistance to marine aggressiveness, abrasion and impacts. Hard and elastic, with porcelainic appearance.
- Resistant to industrial detergents

Guarantee

The information contained in this leaflet is based on our experience and technical knowledge, obtained through laboratory testing and from bibliographic material. DRIZORO reserves the right to introduce changes without prior notice. Any use of this data beyond the purposes expressly specified in the leaflet will not be the Company’s responsibility unless authorised by us. We shall not accept responsibility exceeding the value of the purchased product.

© 2003 DRIZORO S.A. All rights reserved.