MAXMORTER®
SPECIAL CEMENT MIX FOR MAKING ADHESIVE MORTARS

Description

MAXMORTER is a specially formulated cement and additive base which when mixed with the suitable sand produces an adhesive mortar for fixing interior tiles without the need of applying a levelling render beforehand.

Application

- Over even or uneven surfaces, does not require prior levelling.
- For setting mosaics, floor and wall tiles, ceramics, paving tiles in thicker applications.
- Interior use.

Advantages

- Formulated with suitable wetting agents, does not require prewetting of surfaces.
- Easy to use.
- Excellent adhesion.
- Thixotrophic reaction and superior elasticity provide excellent performance.
- Non-Shrink, no hairline cracking in thicker applications.

Mixing

Mix one (1) part of MAXMORTER with four (4) parts of sand using sufficient water to obtain a smooth mortar mix. Sand must be free of dust and clay arid of varied granule distribution of between 0 to 3 mm. Do not use uniform or fine sand.

Coverage

Depending on the surface levels, approximately 4 kg/m2 of MAXMORTER per 10 mm. layer.

Packaging

20 kg. sacks.

Storage

Shelf life of unopened sacks in dry covered storage is 12 months.

Guarantee

The information contained in this leaflet is based on our experience and technical knowledge, obtained through laboratory testing and from bibliographic material. DRIZORO reserves the right to introduce changes without prior notice. Any use of this data beyond the purposes expressly specified in the leaflet will not be the Company’s responsibility unless authorised by us. We shall not accept responsibility exceeding the value of the purchased product.

© 2003 DRIZORO S.A. All rights reserved.