BISEAL® PL
PLASTICISING ADDITIVE FOR CONCRETE AND MORTARS

Description

BISEAL PL is a concentrated plasticiser to improve workability of concrete and mortars

Uses

It is used both for concrete and mortars whether rich or poor in cement content.

Advantages

- High efficiency concentrated product.
- Aids the workability.
- Provides cohesion to the mix, preventing segregation.
- Reduces shrinkage in cement rich mortars and concrete.
- Its slight foaming action breaks the capillary net in mortars and concrete increasing their frost resistance.
- Can be used to reduce the mixing water.

Application instructions

It can be added directly to the mixing water at a rate of 0.1% to 0.2% by weight of cement. Cleaning is done with abundant clean water.

Cautions

- Avoid contact with the eyes and skin.
- Use safety goggles and rubber gloves.
- In case of contact with the skin, wash with luke-warm water and soap.
- In case of contact with the eyes, rinse thoroughly with water seek medical assitance.
- It is a non-flammable product.

Packaging

20 litre jerrycans.

Storage

Twelve months in its original unopened container, in a dry covered place with temperatures above 4ºC.

Consumption

50 cm3 to 100 cm3 per each 50 kg. cement bag.

Technical Data

Density (gr/cm3) at 20ºC | 1.03 ± 0.05
Colour | Yellowish
Solubility in water | Complete
pH | 7 ± 0,5
Appearance | Fluid

Guarantee

The information contained in this leaflet is based on our experience and technical knowledge, obtained through laboratory testing and from bibliographic material. DRIZORO reserves the right to introduce changes without prior notice. Any use of this data beyond the purposes expressly specified in the leaflet will not be the Company’s responsibility unless authorised by us. We shall not accept responsibility exceeding the value of the purchased product.

© 2003 DRIZORO S.A. All rights reserved.