BISEAL® MRL
WATER BORNE MOULD REMOVING LIQUID FOR WOODEN FORMS

Description

BISEAL MRL is an oil emulsyfied in a waterbase, for the removal of wooden plank or board forms, for concrete placed on site.

Uses

Removing of wooden concrete forms.

Advantages

- Easy de-moulding of the concrete element.
- High non-stick effect.
- Good penetration into wood.

Application

Preparation of the substrate. The wood must be dry, free from cement powder, dust, removing any leftovers from previous de-mouldings, and any other foreign matter.

Application. BISEAL MRL allows the addition of up to 10 litres of water per each 25 litres.

The product is applied using a brush, roller or spray gun until the wood is completely soaked, in one or two applications, depending on its absorption. Wait between 15 to 30 minutes before placing the concrete.

Cautions

- Excessive amounts can cause staining of the concrete.
- Make the application homogeneous on the entire mould surface.
- BISEAL MRL is not a toxic product, but when applying keep in mind not to use the hands without the protection of rubber gloves or protective glasses. If the product comes in contact with the eyes, rinse with abundant clean water but do not rub. If the irritation persists, consult a doctor.

Packaging

220 litre drums and 25 litre jerrycan

Storage

Twelve months in its original unopened container, in a dry covered place protected from frost.

Technical data

Density ( kg / dm3) | 0,99 ± 0,01
Colour | Milky

Guarantee

The information contained in this leaflet is based on our experience and technical knowledge, obtained through laboratory testing and from bibliographic material. DRIZORO reserves the right to introduce changes without prior notice. Any use of this data beyond the purposes expressly specified in the leaflet will not be the Company’s responsibility unless authorised by us. We shall not accept responsibility exceeding the value of the purchased product.

© 2003 DRIZORO S.A. All rights reserved.