MAXCLEAR® TOP
TRANSPARENT AND WATER REPELLANT PROTECTION FOR SINGLE-LAYER MORTARS

Description

MAXCLEAR TOP is a transparent and based water, water repellant protection, specially designed for applying over recent single-layer mortars, to prevent the formation of lime efflorescences.

Uses

- Protection of single-layer mortar façades, whether recent or already aged.
- Protection of brick, concrete block, screeds.

Advantages

- Can be applied over recent single-layer mortar applications to the setting be finished.
- It prevents the appearance of lime on single-layer mortars, recently applied, without requiring they be fully set.
- It does not change the appearance of the substrate.
- Reduces water absorption of the façade, protecting it from frost damages.
- Allows the surface to breathe.
- It is self-cleaning by rain, extending the façade's lifetime.
- Provides savings in auxiliary means for further applications on the façade and reduces maintenance costs

Application instructions

Surface preparation. The surface to be treated must be free of dust and foreign elements. It is highly recommended to brush the surface to eliminate any remains of scraping process.

Mixing: Product is ready for use, and does not require any dilution or mixing. It is advisable to stir it a little before applying.

Application: Over recent single-layer mortars, MAXCLEAR TOP must be applied from 24 to 48 hours after application of the mortar, in two successive layers, the second one when the first one has dried. The time varies depending on weather conditions.
On existing single layer mortars, brick or concrete block walls, it is advisable to dampen the substrate slightly and when it starts to dry, the application of the two coats is done, as indicated in the previous paragraph.
Applying can be done from top to bottom, using brush, roll or spray gun up to substrate saturation, specially with the first coat.

Cautions

It is highly recommended to do a test on working area, with the intention of evaluate the final results before definitive applying, specially when it is applied over already aged single-layer mortars, screeds or other substrates.

MAXCLEAR TOP is not toxic, but it is an abrasive compound. When it is applied, must be taken into account to wear protective rubber gloves and glasses. In case one of the components comes in contact with skin, rinse thoroughly with soap and water, but not rub. Seek Medical attention if irritation continues.

Packaging

20 litres jerrycans.

Storage

Twelve months in its original unopened containers, in a dry place at temperatures above 4ºC.

Technical Data

Appearance | Miky liquid
Density (gr./ cm3) | 0,99
Viscosity Ford Cup nº 4 (sg) | 12
pH | 7
Coverage | 1 to 4 m2 per litre

Guarantee

The information contained in this leaflet is based on our experience and technical knowledge, obtained through laboratory testing and from bibliographic material. DRIZORO reserves the right to introduce changes without prior notice. Any use of this data beyond the purposes expressly specified in the leaflet will not be the Company’s responsibility unless authorised by us. We shall not accept responsibility exceeding the value of the purchased product.

© 2003 DRIZORO S.A. All rights reserved.