MAXREST® PASSIVE
AN ANTI-CORROSIVE PROTECTION FOR RE-ENFORCING RODS AND ALL OTHER IRON OR STEEL SURFACES

Description

MAXREST PASSIVE is a single component liquid material, ready to use as protection for re-enforcing rods and other steel and iron surfaces against oxidisation, acid and alkali attack. MAXREST PASSIVE will form part of the oxide as a passive layer giving full protection against corrosion, acid and alkali attack.

Uses

- As anti-corrosive protection for re-enforcing steel in the restoration of structural concrete.
- As protection against attack from strong Chemical Agents.

Application Instructions

Surface preparation
Prior to application clean down affected area using a wirebrush and wash with water.
Application
MAXREST PASSIVE does not require dilution or addition of other materials. Apply by brush, spray gun or by immersing the article to be protected.
Product requirements
Recommended application 8 mē/liter for a thickness of 50 micron DFT.
Curing
Depending on temperature 2 to 3 hours before the application of final coatings. e. g. paints, polyurethane, epoxy or other DRIZORO Products.

Caution

Do not apply at temperatures below 5° C or above 60° C. Tools must be cleaned with water immediately after completion of application.

Technical Data

Solids content: | 40% by volume.
Density: | 1,18+0,02 Kg/liter.
Product requirement | 8 mē/liter of for 50 micron dry film 150 grm/mē.
Fireproofing: | Meets British Standard BS473 Part 7-1971.

Packaging

1 liter and 5 liter cans.

Colour

Milky white.

Guarantee

The information contained in this leaflet is based on our experience and technical knowledge, obtained through laboratory testing and from bibliographic material. DRIZORO reserves the right to introduce changes without prior notice. Any use of this data beyond the purposes expressly specified in the leaflet will not be the Company’s responsibility unless authorised by us. We shall not accept responsibility exceeding the value of the purchased product.

© 2003 DRIZORO S.A. All rights reserved.