MAXLEVEL® L
SELF-LEVELLING LIGHT MORTAR FOR INTERIOR FLOORS TREATMENT

Description

MAXLEVEL "L" is a hydraulic setting mortar, based on cements and light aggregates, blent with synthetic resins and super-fluidificants.
MAXLEVEL "L" mixed with water provides a fluid mortar that levels itself without trowelling after being poured.
MAXLEVEL "L" makes up a low weight slab as the density of the dry material is 1.1 gr/cm³.

Advantages

- It makes up a low weignt slab due to the selection of light aggregates
- High adherence due to the modification of the syntnetic resin
- Stress-free hardening, even in thick layers applied at once

Application

Surface preparation
Remove all desintegrated materials so that only sound substrate remains. The surface must be free of dirt, dust, cement grouts, paint, grease or other foreign materials.
Mixing
Pour 400-500 gr. of water into a clean container and add 1 Kg. of MAXLEVEL "L".
Placing
When placing on weakly absorbing floors, prepare the surface priming with MAXBOND.

Test Data

Apparent density: | 0.6 Kg/dm³
Density of hardened material : | 1.12 Kg/dm³
Pot life : | 1 hour
Hardness of the substrate for placing up to 30 min. : | 24 hours
Hardness of the substrate for placing over 50 min. : | Higher than 48 hours

Storage

12 montns when stored in a cool, dry, and frost free place.

Guarantee

The information contained in this leaflet is based on our experience and technical knowledge, obtained through laboratory testing and from bibliographic material. DRIZORO reserves the right to introduce changes without prior notice. Any use of this data beyond the purposes expressly specified in the leaflet will not be the Company’s responsibility unless authorised by us. We shall not accept responsibility exceeding the value of the purchased product.

© 2003 DRIZORO S.A. All rights reserved.