MAXLEVEL® SUPER
QUICK SETTING SELF-LEVELLING MORTAR FOR INTERIOR FLOOR TREATMENT

Description

MAXLEVEL SUPER is a hydraulic setting mortar, based on cements and aggregates, blended with synthetic resins. MAXLEVEL SUPER mixed with water provides a fluid mortar that levels itself without trowelling after being poured.

Uses

MAXLEVEL SUPER is the suitable product for levelling with high performances is required for interior applications.

Advantages

- Self –levelling. MAXLEVEL SUPER spreads its self, even admits pumping.
- Stress-free hardening, even in thick layers applied at once.
- Suitable application over floor heating system.
- Compensated shrinkage.
- It allows thickness up to 15 mm. per layer.
- Quick setting.

Application

Preparation of the surface: Remove all disintegrated materials so that only sound substrate remains. The surface must be free of dirt, dust, cement grouts, paint, grease or other foreign materials.

Mixing: Pour 4.8 - 5 litres of water into a clean container and add 25 kg of MAXLEVEL SUPER.

Mix with medium agitation (300 - 400 rpm), until a homogeneous mortar without lumps is achieved. Let the mix rest for two minutes and re-mix briefly.

Placing: Before pouring the self-levelling mortar MAXLEVEL SUPER, saturate surface with water, but leave no free-standing water. Pour the fluid mortar over the base and distribute regularly all the layer in a single step. It is advisable employing a depth range to check thickness aplication. Before MAXLEVEL SUPER begins to set, apply a spike roller to eliminate air bubbles.

Caution: Do not apply at temperatures lower than 5 ºC nor if there is a fall in temperature expected within 24 hours after application.
Do not apply at temperatures higher than 35ºC. Do not use curing compounds.
Limits of each section should coincide with contraction or concrete joints on the sub-base of concrete in case they exist. Expansion joints must be respected expressly and sealed with a suitable sealant of the MAXFLEX group.

Consumption

Approximately 1.6 kg/m2 of product per mm. thickness.

Packaging

25 kg. bags.

Storage

12 months in its original container, stored in a cool, dry and frost free place.

Technical Data

Colour: Light grey.
Pot life: 20-40 minutes.
Time to allow pedestrian traffic: Between 3 and 5 hours depending on curing conditions.
Time for placement of finishing: Between 1 and 3 days depending on curing conditions.

Fluidity in shaking table (diameter in mm.) | 220
Mechanical resistances (MPa) | Flexural strength | 1 d | 4.0
7 d | 6.5
28 d | 9.2
Compression strength | 1 d | 16.0
7 d | 25.0
28 d | 33.0
Adhesion (MPa) | For 10 mm. thickness | 28 d | 2.10
Taber abrasion resistance (grs) | H 22 grinder, 1000 cycles, 1kg weight | 3.6

Guarantee

The information contained in this leaflet is based on our experience and technical knowledge, obtained through laboratory testing and from bibliographic material. DRIZORO reserves the right to introduce changes without prior notice. Any use of this data beyond the purposes expressly specified in the leaflet will not be the Company’s responsibility unless authorised by us. We shall not accept responsibility exceeding the value of the purchased product.

© 2003 DRIZORO S.A. All rights reserved.