MAXURETHANE®
POLYURETHANE PROTECTION. HIGHLY RESISTANT TO ATTACK FROM PETROL, DIESEL AND LUBRICATING OILS

Description

MAXURETHANE is a product based on Polyurethane synthetic resins, air cured. It is specially formulated for protecting surfaces from the aggressive pollution of petrol, diesel, fuel oil and lubricating oils. It prevents dusting of floors, stores and parking areas.

Uses

- It seals concrete floors to prevent dusting.
- It is a practical long lasting finish for factory floors, warehouses and parking areas.
- It has strong adhesion, elasticity and is resistant to chemical attack and abrasion.
- It can be applied to wood, metal, tiles, etc.
- Ideal for skating rinks, gymnasiums, discotheques, etc.

Application Method

Surface preparation.
The surface to be treated must be solid, dry, free of dust, grease, etc.
Tools.
MAXURETHANE can be applied by brush, roller, air less or air-brush gun.
Apply MAXURETHANE in two coats. The first coat must be dry before applying the second coat at right angles to the first application. Approximately 8 to 10 hours. Never add solvents as these will impair the final finish.
Curing.
Allow a minimum of 72 hours before putting the floor into service.

Physical Characteristic

Density 20 + 2° C : 0,957 g/cm³
Viscosity 20 + 2° C : 40 seconds, Copa Ford Nº 4
Solids content : 40 ± 2%
Application Time (at 20° C and 60% R. H.): once opened MAXURETHANE has a pot life of THREE Hours. Do not apply in extreme temperatures.
Covering: One litre of MAXURETHANE covers an area of approximately 6-7 m² depending on the texture and porosity of surface.
Chemical resistance: 24, 48 and 72 hours complete immersion tests were carried out to show that MAXURETHANE is resistant to Petrol, diesel, fuel oil and lubricant oils.
MAXURETHANE is also resistant to water, dilute alkalies, calcareous water and cleaning materials.
Flash point > 80° C.

Caution

The edge of the lid and container must be thoroughly cleaned before resealing.
Use MAXSOLVENT to clean tools after the work is finished.

Storage

Approximately 12 month when stored in its original packing, in a cool, dry and frost free place.
MAXURETHANE is an inflammable liquid, so all normal storage, transport and handling precautions for these kind of products should be observed.

Guarantee

The information contained in this leaflet is based on our experience and technical knowledge, obtained through laboratory testing and from bibliographic material. DRIZORO reserves the right to introduce changes without prior notice. Any use of this data beyond the purposes expressly specified in the leaflet will not be the Company’s responsibility unless authorised by us. We shall not accept responsibility exceeding the value of the purchased product.

© 2003 DRIZORO S.A. All rights reserved.