MAXSHEEN® POOL
ACRYLIC COATING FOR SWIMMING POOLS

Description

MAXSHEEN-POOL is a high quality elastic acrylic coating, resistant to both infrared and ultra-violet rays, chafing and algicides and hypochlorites added to swimming pools.

Uses

MAXSHEEN-POOL is applied on concrete floors, cement mortars, etc. Generally, it is applied on building materials used in the production of swimming pools, fountains and dams reservoirs.

Advantages

- It is not toxic.
- Application temperature between 5 deg C minimum and 40 deg C maximum.
- Excellent elasticity.
- Impervious to water and pervious to water steam.
- MAXSHEEN-POOL is fugicide and bactericidal, avoiding formation of algae, fungus, lichen, etc.
- Protects against carbon dioxide, hydrochloric iones and water.

Application Instructions

New swimming pools, dams, fountains, etc.
The surface to be coated must be free from dirt, grease, etc.
When the reservoir has set for 10 days minimum, apply a first coat diluting MAXSHEEN-POOL with 10-20% of water. Allow at least 4-5 hours curing.
Apply a second coat, without diluting, and allow 24 hours curing. Water filling should be done between a minimum of 7 and a maximum of 14 days.
Painted swimming pools, dams, fountains, etc.
Bad adhered paint must be completely eliminated. Sandpaper properly adhered paint.
When the reservoir has set for 10 days minimum, apply a first coat diluting MAXSHEEN-POOL with 10-20% of water. Allow at least 4-5 hours curing, depending on weather condition.
Apply a second coat as it comes from the can and allow 24 hours curing. Water filling should be done between a minimum of 7 and a maximum of 14 days.
MAXSHEEN-POOL can be applied by brush, spray or roller.

Test Data

Density : | 1,15 g/cm³
Solids content : | 76%
PVC : | 30%
Adherence (criss-croas pattern testing) : | Very good. No criss-cross pattern is loose
Touch curing : | 1 hour
Total curing : | 2 hours

Coverage

8-10 m²/Kg. depending on the absorption rate of the surface to be treated.

Packaging

20 Kg. cans

Guarantee

The information contained in this leaflet is based on our experience and technical knowledge, obtained through laboratory testing and from bibliographic material. DRIZORO reserves the right to introduce changes without prior notice. Any use of this data beyond the purposes expressly specified in the leaflet will not be the Company’s responsibility unless authorised by us. We shall not accept responsibility exceeding the value of the purchased product.

© 2003 DRIZORO S.A. All rights reserved.