MAXELASTIC® STONE
PROTECTIVE WEARING SURACE FOR ROOFS AND TERRACES WATERPROOFED WITH MAXELASTIC

Description

MAXELASTIC STONE is a mixture of water-based copolymers and fine graded aggregates. MAXELASTIC STONE is a synthetic mortar ready to be used as a protective layer over MAXELASTIC waterproofing jobs, preventing damages caused by pedestrian traffic. Spreaded by trowel, it will provide a continuous and decorative layer.

Uses

- As a protection of MAXELASTIC against damages caused by pedestrian traffic.
- As a decorative and anti-slip floor.

Advantages

- Non-slip. Resistant to abrasion.
- Fully compatible if installed over MAXELASTIC layers, with no needs of special primers, etc.
- Single-component product, ready to be used.
- Decorative. Available in different colours.

Application

Surface preparation: the surface must be clean and dry, free of any trace of dust or dirt.
If applied directly over MAXELASTIC, MAXELASTIC STONE can be spread once the last layer is dry. (Refer to application instructions in MAXELASTIC Thecnical Bulletin nē 18.00)
When spreaded over concrete or slope forming mortars, apply a previous coat of MAXELASTIC diluted with water (approx 70/30 depending on the porosity of the surface) as a primer.
Spreading: MAXELASTIC STONE is supplied ready to be used. Can be spreaded by means of a trowel, or displaying rules defining the required thicknes. It can be laid at one go with no need to apply more than one layer. To ensure a good and efficient protection, apply a layer minimum 3 mm. average thick, avoiding layers thiner than 2 mm.
Respect every single expansin joint existing in the roof to allow free movements without creating unnecesary stresses. Define small working areas that should be finished in just one go, thus avoiding irregular joints. Smalldefects in the finishing can be masked with an application by brush of MAXELASTIC STONE diluted with water, as if it were a slurry.

Caution

Do not apply below 5ēC or with existing R.H exceeding 90%. Do not apply if rain is expected to fall in the 24 hours after application.

Packing

25 Kg. pails

Colours

Available in grey, tile red and white. Black and green upon request. Other colours upon special request depending on the quantity to be ordered.

Storage

12 months protected from sun and freezing, it its original and unopened pail.

Technical Data

Density: 1,7 kg/dm3
Application requeriment: 4-5 kg m2
For further information concerning the resin, refer to MAXELASTIC Technical Bulletin (nē18.00)

Guarantee

The information contained in this leaflet is based on our experience and technical knowledge, obtained through laboratory testing and from bibliographic material. DRIZORO reserves the right to introduce changes without prior notice. Any use of this data beyond the purposes expressly specified in the leaflet will not be the Company’s responsibility unless authorised by us. We shall not accept responsibility exceeding the value of the purchased product.

© 2003 DRIZORO S.A. All rights reserved.